# Data Processing Order of Operations

1. Get 4 date/times on virtual van/sealog
   * Start of launch (in water)
   * Start of Ops (on bottom)
   * End of Ops (off bottom)
   * On Deck
2. Do h264 transfers
   * Backup h264 machines
3. Offload Sulis camera photos
4. Backup AJA drives (4k and 1080i highlights)
5. Start HDGrabs downloads
6. Pull sensor data/dlog
7. Renav
8. Finish photo/video post processing
9. Update metadata csv
10. Apply renav to virtual van
11. SeaLog Data maintenance
12. Merge watch stander and metadata csv’s
13. Make Jason HTML tree
14. Copy over virtual van
15. Rsync drives
16. Collect Nav comp data from lead navigator (underlays/targets/origin)
17. Collect data from winch computer
18. Complete documentation